TRANSPORT COMPLIANCE  /  FLEET MANAGEMENT
Vehicle Off Road (VOR)
Vehicle withdrawal • Safety inspection checks • Return to service
	01
	VEHICLE TAKEN OFF ROAD



	VEHICLE REGISTRATION
 
	DATE TAKEN OFF ROAD
 
	ODOMETER READING (KM)
 



Reason vehicle taken off road





	AUTHORISED BY / SIGNATURE
 
	PRINT NAME
 
	DATE
 



	02
	RETURN TO SERVICE — SAFETY INSPECTION



	DATE OF LAST SAFETY INSPECTION (SI)
 
	WEEKS SINCE LAST SI
 
	AGREED SI INTERVAL (WEEKS)
 



Safety inspection required before return?   ☐ Yes     ☐ No
	IF YES, DATE SI COMPLETED
 
	SI RECORD / REFERENCE
 



IMPORTANT — SAFETY INSPECTION REQUIREMENT
Check the date of the last Safety Inspection before returning the vehicle to service. If the agreed inspection interval has been exceeded, a Safety Inspection must be completed and any defects repaired before the vehicle is used. Failure to do so may breach operator licence undertakings and put the operator’s licence at risk.
	03
	VEHICLE RETURNED TO SERVICE



	DATE RETURNED TO SERVICE
 
	ODOMETER READING (KM)
 



If the odometer reading differs from the VOR reading, explain why




	AUTHORISED BY / SIGNATURE
 
	PRINT NAME
 
	DATE
 




RECORD CONTROL
Retain this form in the vehicle file between safety inspections to explain any gap in the safety inspection history.	
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